{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":7,"rows_kept":12,"merged":[[1,0,6,0],[1,6,6,6],[8,0,9,0]],"flags":["formulas_cached_only"]}
["申请科室","设备名称","数量","单位","预算单价（元）","预算总金额（元）","参数备注"]
["消毒供应中心","清洗消毒器",2,"台",1000000,2000000,"现场查勘"]
[null,"眼科专用真空清洗机",1,"台",300000,300000]
[null,"医用真空快风干燥柜",1,"台",300000,300000]
[null,"环氧乙烷灭菌器",1,"台",1500000,1500000]
[null,"蒸汽清洗工作站",1,"台",95000,95000]
[null,"脉动真空灭菌器",1,"台",2000000,2000000]
["肝胆外科","内窥镜图像处理装置",1,"台",86000,86000,"1.内窥镜处理装置可与电子内窥镜配套使用（包括一次性使用电子胆道成像导管等）；\n2.具有增益功能，通过电子增益的方式，调节图像亮度；\n3.电子内窥镜成像导管，前端LED提供照明;视场角≥120°；全长为700mm-800 mm，工作长度为380mm-400mm；成像导管头部弯曲角度向上≥180°，向下≥180°；景深范围0.5mm～120mm;\n4.双注水通道，工作通道≤1.2mm，内窥镜成像导管直径≤10.8Fr（3.6mm）。\n\n"]
["重症医学科","支气管镜",2,"台",90000,180000,"用于重症患者床旁呼吸道检查及治疗"]
[null,"可视喉镜",1,"套",98000,98000,"用于重症患者床旁气道检查"]
["麻醉科","超声诊断系统",2,"台",400000,800000,"用于疼痛患者的超声引导治疗"]
["内分泌科","胰岛素泵",4,"台",32000,128000,"用于糖尿病患者的胰岛素精准治疗"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}