{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":4,"n_cols":8,"rows_kept":4,"flags":["formulas_cached_only"]}
["序号","申请科室","项目名称","数量","单位","单价（万\n元）","总价（万元）","参数备注"]
[1,"医学工程部","医用气体",1,"年",350,350,"1.提供符合国家规范要求医用气体（液态氧、桶装液氧、氧气、二氧化碳、氮气、液氮、氩气、氦气等）供应、运输、二次搬运至招标人指定位置，且提供与之配套的罐、瓶供采购人免费轮流使用，中标人负责储罐与钢瓶的定期检测，保证钢瓶的安全使用。\n2.严格执行国家质量安全标准，符合《中华人民共和国药典》要求，医用气体纯度≥99.5%，气体生产企业有中华人民共和国药品生产许可证、药品注册证或药品注册证批件、中华人民共和国危险化学品经营许可证、中华人民共和国道路运输经营许可证、气瓶充装许可证。\n3.投标人应具备多车辆送货，中标人每次送货需要到采购人贮罐现场进行专业性供气安全检查和供气技术指导，需确保氧气加注安全。\n4.投标人的投标分项报价表中的数量，为1年预估的需求量，单价为每批次的采购结算单价，采购人每批次采购时，按实际需求量进行采购，结算按照每批次实际用量*采购单价结算。在合同有效期内双方不得以任何理由向上调整价格。\n5.安排至少1名专职人员驻院帮助院方在院内搬运瓶装医用气体。\n6.提供瓶装氧气管理信息系统一套。"]
[2,"内分泌科","掌式超声显像仪",1,"台",9.5,9.5,"1.用于检测糖尿病人皮下组织超声波检测；\n2.掌上类PAD型，便于携带；\n3.至少携带超声探头一只。"]
[3,"口腔科","电动抽吸机（泵）",1,"台",9,9,"1.用于医院或牙科诊所的牙科治疗设备在作钻牙等的治疗时，吸取喷雾、唾液、血液及小颗粒时的抽吸动力源，同时具有分离水气及自动排放功能；\n2.满足8-10台牙椅同时使用，可达24 L/min，可处理含70%泡沫液体，并可同时处理痰盂下水，可达22860 r/min，一体化组合式湿抽结构（即抽吸泵与分离器同轴）；\n3.可直接与牙科治疗机相连接，内置的水泵不断的排除液体，无需水循环等功能。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}