{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet2"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"merged":[[0,1,0,6],[26,1,26,6],[27,1,27,6]],"flags":["formulas_cached_only"]}
[null,"2025年苏北人民医院不干胶、热敏纸采购需求明细"]
["序号","物品名称","型 号","技术参数及要求","数量","单位","备注","样品"]
[1,"热敏不干胶\n","80mm*50mm（850张）","★三防热敏纸模切带撕裂线、间歇3mm、贴试剂管不起敲、强黏不脱落、防划擦不变色 (纸管内径25mm)",6800,"卷","各病区","提供样品1卷"]
[2,"热敏不干胶\n提供样品1卷","50mm*30mm（2000张）","★三防热敏纸模切带撕裂线、间歇3mm、贴试剂管不起敲、强黏不脱落、防划擦不变色 (纸管内径25mm)",3300,"卷","各病区","提供样品1卷"]
[3,"热敏不干胶","45mm*30mm（2000张）","三防热敏纸模切带撕裂线、间歇3mm、强黏不脱落、防划擦不变色 (纸管内径25mm)",15,"卷"]
[4,"热敏不干胶","70mm*50mm（500张）","三防热敏纸模切带撕裂线、间歇3mm、强黏不脱落、防划擦不变色 (纸管内径4cm)",350,"卷"]
[5,"热敏不干胶\n提供样品1卷","85mm*40mm（1200张）","★三防热敏纸、蓝色格拉辛底纸、模切带撕裂线、间歇3mm、右上角模切40*20可撕角、贴试剂管不起敲、强黏不脱落、撕去胶水无残留、防划擦不变色 (纸管内径25mm)",600,"卷","检验科","提供样品1卷"]
[6,"热敏不干胶\n提供样品1卷","80mm*70mm（5000张）","★特防热敏合成纸、不带撕裂线、间歇3mm、自动贴签机专用、防静电、防腐蚀、撕去胶水无残留、防划擦不变色 (纸管内径76mm)",90,"卷","pivas","提供样品1卷"]
[7,"热敏不干胶","77mm*45mm（200张）","双色印刷（印医废标识）三防热敏纸、间歇3mm、强黏粘贴不起敲、防划擦不变色 (纸管内径25mm)",600,"卷"]
[8,"热敏不干胶\n提供样品1卷","50mm*30mm（2000张）","★三防热敏纸模切带撕裂线、间歇3mm、耐高温120度不变色、不脱落、防划擦不变色 (纸管内径25mm)",20,"卷","中药房","提供样品1卷"]
[9,"PET不干胶","90mm*60mm（1000张）","带撕裂线、间歇3mm、贴在棉布及无纺布上、耐高温200度不脱落、不变色、胶水无残留(纸管内径25mm)",10,"卷"]
[10,"PET不干胶","65mm*42mm(1000张)","带撕裂线、间歇3mm、贴在棉布及无纺布上、耐高温200度不脱落、不变色、胶水无残留(纸管内径25mm)",300,"卷"]
[11,"PET不干胶\n提供样品1卷","55mm*35mm(1000张)","★带撕裂线、间歇3mm、贴在棉布及无纺布上、耐高温200度不脱落、不变色、胶水无残留(纸管内径25mm)",400,"卷","消毒供应中心","提供样品1卷"]
[12,"PET不干胶","74mm*44mm(1000张)","亚银材料、带撕裂线、间歇3mm、强黏粘贴不起敲、不变色、防腐蚀、防划擦(纸管内径25mm)",50,"卷"]
[13,"铜版纸不干胶\n提供样品1卷","28mm*24mm(5000张)","★带撕裂线、间歇3mm、强黏不脱落   空白  (纸管内径25mm)",50,"卷","病理科","提供样品1卷"]
[14,"铜版纸不干胶\n提供样品1卷","80mm*80mm(1000张)","★可移不干胶撕去胶水无残留、带撕裂线、粘贴不脱落    空白 (纸管内径25mm)",200,"卷","pivas","提供样品1卷"]
[15,"铜版纸不干胶","管道标识80mm*15mm（200张）","约50种标识，按实际内容印刷，满底色+黑色文字、间歇2mm、强黏不脱落、不掉色(胶管内径30mm)",1000,"卷"]
[16,"碳  带","80mm*70m","全树脂热转印碳带、防酒精、防刮磨、不褪色(纸管内径12mm)",450,"卷"]
[17,"碳  带","100mm*300m","全树脂热转印碳带、防酒精、防刮磨、不褪色(纸管内径25mm)",25,"卷"]
[18,"碳  带","110mm*90m","全树脂热转印碳带、防酒精、防刮磨、不褪色(纸管内径12mm)",20,"卷"]
[19,"床头插卡","105mm*45mm","约10种内容，按实际内容印刷，不干胶满底色+黑色文字或镂空文字、不掉色、复合厚度1.5mm单面磁铁",1000,"个"]
[20,"热敏纸","80mm*80mm","宽80mm、直径≥78mm、热敏纸厚度≥0.06mm(胶管内径24mm)",18000,"卷"]
[21,"热敏纸","57mm*35mm","宽57mm、直径≥35mm、热敏纸厚度≥0.06mm(胶管内径12mm)",400,"卷"]
[22,"热敏纸","110mm*50mm","宽110mm、直径≥47mm、热敏纸厚度≥0.06mm(胶管内径24mm)",500,"卷"]
[23,"热敏纸","210mm*295mm\n200张/本","迈瑞心电图机专用",800,"本"]
[24,"热敏纸","63mm*30m","心电图机专用，三导",600,"卷"]
[null,"提供材料\n检测报告：符合ROHS新标准2011/65/EU及其修订指令（EU）2015/863中汞、铅、镉、多溴联苯、邻苯二甲酸二丁酯、邻苯二甲酸二异丁酯、六价铬、多溴联苯醚等有害物质含量要求的限值。\n"]