{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":7,"n_cols":7,"rows_kept":7,"flags":["formulas_cached_only"]}
["序号","申购科室","设备名称","数量\n（台套）","单价\n（万元）","总额\n（万元）","功能需求"]
[1,"推拿科","颈、腰椎牵引装置",2,9.9,19.8,"1.治疗颈椎病及腰椎间盘突出的牵引装置；                     2.能够单独进行颈椎、腰椎牵引，能够随时暂停或取消牵引工作，参数及牵引模式可调节，不需要加热功能。"]
[2,"内镜诊治中心","内镜清洗机",2,9.8,19.6,"用于软式内镜的清洗与消毒灭菌"]
[3,"耳鼻咽喉头颈外科","清洗工作站",1,10,10,"1.用于软式内镜清洗与消毒灭菌；                                2.硬镜、器械等的清洗与消毒；                             3.需要按现有尺寸定制。                               "]
[4,"骨科","医用放大镜和手术辅助照明灯",2,9.9,19.8,"1.LED头灯，光照不低于68000Lux, 色温不低于6000K，LED明亮纯白光；\n2.便携式充电锂电池的应用，不低于6小时；\n3.放大镜倍数有2.5X ，3.0X ,3.5X ,4.5X等，可供临床选择。"]
[5,"消毒供应中心","蒸汽枪工作站",1,9.5,9.5,"1.用于清洗手术器械、微创器械、管腔器械、硬式内窥镜等器械的清洗；                        2.具有安全保护功能；                               3.设备水槽需要现场定制。                  "]
[6,"公共卫生管理科","一氧化碳测量仪",1,1.2,1.2,"1.能够准确检测吸烟者呼出的肺部一氧化碳。\n2.量程与精度能够覆盖从非吸烟者到重度吸烟者的检测需求。\n3.确保能够检测到微小的一氧化碳浓度变化，测量精度可达 ±0.1ppm。\n4.传感器寿命：大于12个月，减少更换频率，降低维护成本。\n5.屏幕液晶显示，清晰展示检测结果。\n6.具备数据存储功能或支持PC端数据管理软件，便于进行数据分析和患者管理。"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}